The latest lab file on our download server, "fritzrepeater-XXXX-Labor-xxxx.zip", contains
- the lab version for your FRITZ!Repeater
- this "infolab-en.txt" file with important information on this lab version
- information, feedback options, and the file at en.fritz.com/fritz-lab


New and improved with FRITZ!OS 8.24

- NEW: Smart Networking (1)
- NEW: Simplified access to the user interfaces of FRITZ!Repeaters (2)
- Improvement - There is no reboot required anymore when language or country are changed
- several corrections and stability improvements


(1) Smart Networking
In a home network consisting of a FRITZ!Box and more than one FRITZ!Repeater, the W-Fi connections of the repeaters are re-evaluated and optimized whenever changes are made in the home network or a repeater is restarted. Example: A FRITZ!Repeater is already connected to the home network. A second FRITZ!Repeater is added and connected directly to the FRITZ!Box. It can then be moved and plugged into the desired location. The repeaters now re-evaluate the situation and decide whether the new repeater should connect to the first repeater, or whether it should remain connected to the FRITZ!Box.
Requirement: FRITZ!OS 8.20 or newer is installed on the FRITZ!Box and all of the FRITZ!Repeaters. This option can be disabled in the FRITZ!Box user interface under 'Home Network > Mesh > Mesh Settings'.

(2) Simplified access to the user interfaces of FRITZ!Repeaters
When switching from the FRITZ!Box user interface to the user interface of a FRITZ!Repeater in the Mesh, it is not necessary to re-enter any login data (single-sign-on).
Requirement: FRITZ!OS 8.20 or newer is installed on the FRITZ!Box and all of the FRITZ!Repeaters.

------------------------------------------------------------
# Improvements within FRITZ!Labor with -133871

Fixed: Internet access could potentially be lost after running for a period of time
Fixed: Automatic optimization of the connection between the repeater and another repeater was not triggered reliably
Fixed: The 5 GHz Wi-Fi connection was not restored in some cases following radar detection
Improvement: Stability improvements


# Improvements within FRITZ!Labor with -133387
Fixed - After a radar detection, the 5 GHz connection to the FRITZ!Box was sometimes reestablished with 20 MHz


# Improvements within FRITZ!Labor with -133127
Fixed - Temporary loss of data traffic between FRITZ!Repeater and FRITZ!Box

# Improvements within FRITZ!Labor with -132446

Fixed - The UI diagnostic tool could falsely indicate a missing internet connection
Fixed - Resolved an issue occasionally causing incorrect operating modes in daisy-chained FRITZ!Repeater setups
Improvment - Wi-Fi stability improved


# Improvements within FRITZ!Labor with -132119

Fixed - Several textual fixes for the user interface
Improved - Stability improvements


Verbesserungen mit Laborversion -132119

Behoben - Kleinere Fehlerkorrekturen in der Benutzeroberfläche
Verbesserung - Stabilitätsverbesserung


# Improvements within FRITZ!Labor with -131593

Fixed - When using a device with Wi-Fi 7, no connections with MLO were displayed under "Wi-Fi connection" in the properties of the network device 
Improvement - When using LAN clients with incompatibilities to EEE (energy efficient ethernet), the feature can be disabled on the support page of the user interface
Improvement - Stability improvements



# Improvements within FRITZ!Labor with -131103

Fixed - When the Wi-Fi connection to the router was lost, the connection on 5 GHz was not reestablished in some cases
Fixed - Channel bandwidth could be limited to 80 MHz in the 5-GHz band after a restart
Fixed - After changing country and time zone, the time stamp in the user interface was not updated
Fixed - Improved translations


# Improvements within FRITZ!Labor with -130557

first FRITZ!Labor version

------------------------------------------------------------
Additional Feedback on FRITZ!OS
======================================

In addition to direct feedback in our lab area en.fritz.com/fritz-lab, there is an additional feedback function in the user interface which provide information. We have automated the processing of feedback supplied by this function.

Wi-Fi feedback via "Wi-Fi / Wi-Fi Network": Feedback icon after the clients

Information on the Lab update:
============================

This FRITZ! Lab firmware is a beta version. We've tested it in standard environments before release, but it may still result in bugs. FRITZ is not liable for any damages that may arise from the use of the Lab version.

Information on working with Lab versions

We appreciate any feedback from our users, which can be submitted at: en.fritz.com/fritz-lab. This page also lists all of the current FRITZ! Lab versions with corresponding feedback areas.

Before you start testing the Lab version

1) You haven't installed the latest firmware for your FRITZ!Box yet? You first need to update the firmware to the latest release.
2) Save your current settings under "System / Backup". The saved settings will be needed if you want to switch back from the Lab firmware back to the release firmware.


Testing the Lab version

Once the latest FRITZ!OS version has been installed on your FRITZ!Repeater and you've saved your current settings, you can begin testing.

1) Unzip the "fritzrepeater-yyyy-LabBETA-xxxxx.zip" file.
2) Use the FRITZ!Repeater user interface to install the update:
- Select "View: Advanced" in the footer.
- Click "Update" in the "System" menu.
- Switch to the "FRITZ!OS File" tab.
- Follow the instructions displayed on the screen.
- Enter the path to the Lab firmware and the name of the Lab file (FRITZ.Repeater_xxxx-0x.xx-xxxxx-Labor.image) in the input field.
3) The Lab version is installed on the FRITZ!Repeater. The FRITZ!Repeater will then restart.


Restoring your device to how it was before testing
You can switch back to the official FRITZ!OS at any time under "System > Update > FRITZ!OS Version" or reset the FRITZ!Repeater back 
to the official FRITZ!OS using the enclosed Windows program "recover.exe" (included in the Lab package).

_________________________________________________________

  FRITZ GmbH 2026. All rights reserved.

This FRITZ firmware package contains files that are distributed under various licenses, in particular under an proprietary license 
or an open-source license (GNU General Public License, GNU Lesser General Public License or FreeBSD License). For details on the various 
licenses, see the "license.txt" file (https://download.avm.de/fritzbox/license.txt).
The source code of the files distributed as open source can be requested in writing to fritzbox_info@avm.de.

FRITZ grants the non-exclusive right to use this firmware package, which is supplied exclusively in object code format. 
The licensee may create only one copy of the software, which may be used exclusively for backup purposes.
FRITZ reserves all intellectual property rights except as expressly granted herein. In particular, without previous approval in writing 
and except as permitted by law, this FRITZ firmware packet may not be reproduced, distributed or in any other manner made publicly accessible, nor may it be edited, disassembled, reverse engineered, translated, decompiled or otherwise "opened" in whole or in part, and subsequently reproduced, distributed or made publicly accessible
_________________________________________________________
KSH 061826